**SPECIFICATION SHEET **

GD BACK PAINTED AND SPLASHBACKS

Using the Makor automated four gun glass coating system Glass Design Back Painted Glass gives architects, builders, designers and homeowners a glass product that is extremely flexible to work with. Ideal for kitchens, bathrooms and splash backs, back painted glass is normally applied to Low Iron glass between 6-19 mm thicknesses and toughened to BS6206 class A.

* Choice of any [RAL or DULUX](http://www.glass-design.net/Back_Painting) RAL or Dulux colour
* Cost effective
* Almost every type of glass can be coated
* Easily cleaned
* No grouting required - Easy to follow [installation](http://www.glass-design.net/Back_Painting) guide
* Durable and heat resistant
* Can be cut or drilled to accommodate fixtures and fittings
* Colourfast, and non-staining
* Minimal joins required
* Reduced wall preparation
* Consistent colour
* Available in large sizes  1700 x 3200 mm

Available: Glass Designs Ltd

 Contract Shower Division

 Unit 3-4 City Cross

 Salutation Road

 London SE10 0AT

 0208 858 8050

 Email: info@glass-designs.net

 Web: [www.glass-designs.net](http://www.glass-designs.net)

 Web: www.glassdesignshowers.co.uk